\hypertarget{filterDesign_8hpp}{}\section{filter\+Design.\+hpp File Reference}
\label{filterDesign_8hpp}\index{filter\+Design.\+hpp@{filter\+Design.\+hpp}}


This file contains code for performing filter design.  


{\ttfamily \#include $<$S\+P\+L/config.\+hpp$>$}\\*
{\ttfamily \#include $<$S\+P\+L/\+Sequence1.\+hpp$>$}\\*
\subsection*{Functions}
\begin{DoxyCompactItemize}
\item 
Real\+Sequence1 \hyperlink{group__Filter__design_gaab880db5d7d30b971c5faa705758ca76}{S\+P\+L\+::lowpass\+Filter} (double cutoff\+Freq, double trans\+Width, double max\+Passband\+Ripple=0.\+1, double min\+Stopband\+Atten=20.\+0)
\begin{DoxyCompactList}\small\item\em Design a zero-\/phase F\+I\+R lowpass filter. \end{DoxyCompactList}\item 
Real\+Sequence1 \hyperlink{group__Filter__design_ga22cf54591e73dfc72b3386ebdb3f9ed7}{S\+P\+L\+::highpass\+Filter} (double cutoff\+Freq, double trans\+Width, double max\+Passband\+Ripple=0.\+1, double min\+Stopband\+Atten=20.\+0)
\begin{DoxyCompactList}\small\item\em Design a zero-\/phase F\+I\+R highpass filter. \end{DoxyCompactList}\item 
Real\+Sequence1 \hyperlink{group__Filter__design_ga6402cb495afbdabd057d0553f833a95a}{S\+P\+L\+::bandpass\+Filter} (double cutoff\+Freq0, double cutoff\+Freq1, double trans\+Width0, double trans\+Width1, double max\+Passband\+Ripple=0.\+1, double min\+Stopband\+Atten=20.\+0)
\begin{DoxyCompactList}\small\item\em Design a zero-\/phase F\+I\+R bandpass filter. \end{DoxyCompactList}\end{DoxyCompactItemize}


\subsection{Detailed Description}
This file contains code for performing filter design. 

